<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.28.2-Firenze">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["Xian 1980 / Gauss-Kruger zone 19",BASEGEOGCRS["Xian 1980",DATUM["Xian 1980",ELLIPSOID["IAG 1975",6378140,298.257,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4610]],CONVERSION["6-degree Gauss-Kruger zone 19",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",111,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",1,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",19500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["northing (X)",north,ORDER[1],LENGTHUNIT["metre",1]],AXIS["easting (Y)",east,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Topographic mapping (medium scale)."],AREA["China - onshore between 108°E and 114°E."],BBOX[18.11,108,45.11,114]],ID["EPSG",2333]]</wkt>
      <proj4>+proj=tmerc +lat_0=0 +lon_0=111 +k=1 +x_0=19500000 +y_0=0 +ellps=IAU76 +units=m +no_defs</proj4>
      <srsid>302</srsid>
      <srid>2333</srid>
      <authid>EPSG:2333</authid>
      <description>Xian 1980 / Gauss-Kruger zone 19</description>
      <projectionacronym>tmerc</projectionacronym>
      <ellipsoidacronym>EPSG:7049</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
